USB Mass Storage support registered.

hub 1-3:1.0: USB hub found

hub 1-3:1.0: 4 ports detected

usb 1-3.2: new full speed USB device using address 4

scsi0 : SCSI emulation for USB Mass Storage devices

Vendor: MITSUMI Model: USB FDD Rev: 1050

Type: Direct-Access ANSI SCSI revision: 02

USB Mass Storage device found at 4

usb 1-3.3: new high speed USB device using address 5

scsi1 : SCSI emulation for USB Mass Storage devices

Vendor: DVDRW Model: USB1008UI Rev: 0057

Type: CD-ROM ANSI SCSI revision: 02

Attached scsi removable disk sda at scsi0, channel 0, id 0, lun 0

USB Mass Storage device found at 5

sr0: scsi3-mmc drive: 1x/40x writer cd/rw xa/form2 cdda tray

Attached scsi CD-ROM sr0 at scsi1, channel 0, id 0, lun 0

ACPI-0405: *** Error: Handler for [EmbeddedControl] returned AE_BAD_PARAMETER

ACPI-1133: *** Error: Method execution failed [\_SB_.ADP1._PSR] (Node df5d66e0), AE_BAD_PARAMETER

ACPI-0405: *** Error: Handler for [EmbeddedControl] returned AE_BAD_PARAMETER

ACPI-1133: *** Error: Method execution failed [\_SB_.BAT1._STA] (Node df5d6760), AE_AML_NO_RETURN_VALUE

ACPI: Power Button (FF) [PWRF]

ACPI: Sleep Button (CM) [SLPB]

EXT3 FS on dm-0, internal journal

cdrom: open failed.

kjournald starting. Commit interval 5 seconds

EXT3 FS on hda2, internal journal

EXT3-fs: mounted filesystem with ordered data mode.

Adding 1015800k swap on /dev/VolGroup00/LogVol01. Priority:-1 extents:1

usb 1-1: string descriptor 0 read error: -71

usb 1-1: string descriptor 0 read error: -71

usb 1-1: string descriptor 0 read error: -71

usb 1-1: string descriptor 0 read error: -71

usb 1-1: string descriptor 0 read error: -71

usb 1-1: string descriptor 0 read error: -71

parport0: PC-style at 0x378 (0x778) [PCSPP,TRISTATE,EPP]

parport0: irq 7 detected

ieee1394: Initialized config rom entry `ip1394'

ip_tables: (C) 2000-2002 Netfilter core team

2005-08-30T20:56:23